**1: gen image SD**


制作SD卡镜像

Open win32diskimager.exe, Load the image data “7500N-myd-y6ull-20240912.rootfs.sdcard”

(The name maybe is update-emmc-xxxxxxxxx.rootfs.sdcard)


打开win32diskimager.exe，加载镜像文件“7500N-myd-y6ull-20240912.rootfs.sdcard”

（名称可能是update-emmc-xxxxxxxxx.rootfs.sdcard）




Run “write in ” button to write the image data into SD.


运行“写入”按钮，将数据写入SD。



Press “Yes” to continue.

按“Yes”继续





**2: recover SP7500N**

Step1: depart the model

拆开机器




Step2: remove the top board (power board) and set the switch of the core board.

Insert the SD that has image data.

Set the switch like following (recovery way).

拆开电源板，插入SD卡，并且将拨码盘设置如下



Then put the top board (power board), and power on, **make sure wait more than 3 minutes, and recovery will be over!**

然后装上顶板（电源板），打开电源，确保等待3分钟以上，恢复结束！

Step3: Set the switch like following (the default way) , then assemble the whole model.

按照以下方式设置拨码（默认工作方式），然后组装整个模型。

